DC outline for documenting procedures

Where NOT to put things

13-15

24-26

39-top

PDU

A, B, C, D

uprights placement for new (30A) PDUs (bottom to top) should be 28 1/8’ apart and plumb

numberd reverse from 20A PDU (top to bottom)

S/N and asset number collection

MAC address

Network (on switch)

Admin => even (clip down)

NFS => odd (clip up)

Others go by the spreadsheet….

Cabling

Color

Dressing